**Exclusive Specification**

**ACCU SYNC**

Fixed and adjustable regulators shall be threaded directly onto the valve

* Adjustable ACCU SYNC shall provide downstream pressure regulation from 20-100 PSI
* Fixed pressure ACCU SYNC’s shall provide either 30 PSI (2 bar; 206 kPa) or 40 PSI (2.56 bar; 276 kPa) downstream pressure
* 40 PSI (2.56 bar; 276 kPa) regulator shall be clearly marked with gray color
* 30 PSI (2 bar; 206 kPa) regulator shall be clearly marked with red color
* Adjustable ACCU SYNC shall display pressure with PSI on one side and BAR on the other
* Adjustable ACCU SYNC shall be adjustable from coined twist knob on end of body
* Adjustable ACCU SYNC shall provide indication of pressure through clear viewing window
* Regulators shall work with both Hunter AC and DC-latching solenoids
* Regulators shall work on ALL Hunter valves at ANY suggested flows